Steps to flash LAN EEPROM:

	Linux_x64,
		1. Make sure to have admin privilege.
		2. If install, FWUpdate.sh and nvmupdate64e are NOT executable, run "chmod +x install FWUpdate.sh nvmupdate64e".
		3. To install the tool. run "./install". 
		4. To update FW, run "./FWUpdate.sh".
		5. Reboot.